|  |  |  |  |
| --- | --- | --- | --- |
| Heavy Duty Post Protectors Protects pallet racks against forklift abuse. Made of heavy 7 gauge steel. Base plate is 8"W x 6"D, with a 4" column opening. 5/8" anchor holes are provided for a 1/2" diameter wedge anchors (supplied by others). Durable yellow powder coat finish. Taller post protectors available. Contact dealer for availability and pricing. Made in USA. FOB Chicago, IL 60639. | |  | |
| **Product No.** | **Length** | | **Weight (lbs.)** |
| TP-12  TP-18  TP-24 | 12”  18”  24” | | 10  16  25 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Snap-On Upright Protectors**   * **Easy Snap-On Installation** * **No Anchoring Required** * Reliable, tough and resilient BALLISTICS grade polymer. * Retains its shape, ensures long & effective lifetime service. * Fits all makes of pallet racking | | |  | | |
| Cost effective protection for your racking. Reduces racking damage by as much as 80%, saving time, trouble, & money. Easy snap-on installation, fits in seconds, no tools or anchoring required. Virtually unbreakable in temperatures above 41°F and operates down to -40°F. Impervious to moisture, mold growth, corrosion, acid, alkaline, and most solvents. High visibility color with other colors available - quantity sensitive. Fully recyclable and non-toxic. Made in USA.FOB Chicago, IL 60639. | | | | | |
| **Product No.** | **Height** | **Column Size**  **W x D** | | **Weight (lbs.)** | **Finish** |
| RAG-A  RAG-B  RAG-C | 23 ½”  23 ½”  23 ½” | 3” x 1-5/8”  3” x 3”  3-3/16” x 2-3/8” | | 2.6  3.3  3.6 | Yellow  Yellow  Yellow |