|  |  |
| --- | --- |
| Heavy Duty Post ProtectorsProtects pallet racks against forklift abuse. Made of heavy 7 gauge steel. Base plate is 8"W x 6"D, with a 4" column opening. 5/8" anchor holes are provided for a 1/2" diameter wedge anchors (supplied by others). Durable yellow powder coat finish. Taller post protectors available. Contact dealer for availability and pricing. Made in USA. FOB Chicago, IL 60639. |  |
| **Product No.** | **Length** | **Weight (lbs.)** |
| TP-12TP-18TP-24 | 12”18”24” | 101625 |

|  |  |
| --- | --- |
| **Snap-On Upright Protectors*** **Easy Snap-On Installation**
* **No Anchoring Required**
* Reliable, tough and resilient BALLISTICS grade polymer.
* Retains its shape, ensures long & effective lifetime service.
* Fits all makes of pallet racking
 |  |
| Cost effective protection for your racking. Reduces racking damage by as much as 80%, saving time, trouble, & money. Easy snap-on installation, fits in seconds, no tools or anchoring required. Virtually unbreakable in temperatures above 41°F and operates down to -40°F. Impervious to moisture, mold growth, corrosion, acid, alkaline, and most solvents. High visibility color with other colors available - quantity sensitive. Fully recyclable and non-toxic. Made in USA.FOB Chicago, IL 60639. |
| **Product No.** | **Height** | **Column Size****W x D** | **Weight (lbs.)** | **Finish** |
| RAG-ARAG-BRAG-C | 23 ½”23 ½”23 ½” | 3” x 1-5/8”3” x 3”3-3/16” x 2-3/8” | 2.63.33.6 | YellowYellowYellow |