|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Teardrop Pallet Rack & Beams**   * Heavy duty steel in all upright frames * Engineered and built for safe, sturdy support * Teardrop style allows for interchangeability of beam sized * Welded green uprights and orange beams are in stock   Made in USA. *FOB Chicago, IL 60639.* | |  | | |
| **TEAR DROP ROLL FORM – OPEN BACK UPRIGHTS** | | | | |
| **Product**  **No.** | **Size**  **D x W** | | **Wt.**  **(lbs.)** | **Cap.\*\***  **(lbs.)** |
| FS08-24-96 | 24 x 96” | | 41 | 16,200 |
| FS08-36-96  FS08-36-144 | 36 x 96”  36 x 144” | | 45  66 | 16,200  16,200 |
| FS08-42-96  FS08-42-120  FS08-42-144  FS20-42-168  FS20-42-192  FS20-42-240 | 42 x 96”  42 x 120”  42 x 144”  42 x 168”  42 x 192”  42 x 240” | | 47  57  69  95  110  145 | 16,200  16,200  16,200  23,200  23,200  23,200 |
| FS08-48-96  FS08-48-120  FS08-48-144  FS20-48-192  FS20-48-240 | 48 x 96”  48 x 120”  48 x 144”  48 x 192”  48 x 240” | | 49  57  71  114  141 | 16,200  16,200  16,200  23,200  23,200 |

|  |  |  |  |
| --- | --- | --- | --- |
| **TEAR DROP BEAMS** | | | |
| **Product**  **No.** | **Length** | **Wt.**  **(lbs.)** | **Cap.\*\***  **(lbs.)** |
| SB3016-048 | 48” | 11 | 6,437 |
| SB3016-096  SB3716-096  SB4116-096  SB4616-096 | 96”  96”  96”  96” | 20  22  24  26 | 3,017  4,409  5,220  5,953 |
| SB4116-108  SB5016-108 | 108”  108” | 27  31 | 4,314  6,344 |
| SB4616-120  SB5016-120 | 120”  120” | 32  42 | 4,517  5,661 |
| SB5556-144  SB6014-144 | 144”  144” | 43  54 | 4,810  6,588 |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Accessories** | | | | |
| **Crossbars** | **Product No.** | **Length** | **Wt. (lbs.)** | **Finish** |
| SR10106FSG  SR10112FSG | 6”  12” | 2  4 | Galvanized  Galvanized |
| **Row Spacers** | **Product No.** | **Length** | **Wt. (lbs.)** | **Finish** |
| SR2016-36DFG  SR2016-42DFG  SR2016-48DFG | 36”  42”  48” | 5  6  7 | Galvanized  Galvanized  Galvanized |
| **Standard Size**  **Accessories** | **Shims** | | **Anchors** | |