|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Pallet Rack Storage System Kits**   * One Starter Unit to begin each row. Add-On Units to extend or complete row. * Unit Widths are 8'-0", 9'-0", and 10'-0". * Unit Depths are 42" or 48". Call for pricing on 36". * Uprights: 8'-0", 10'-0", or 12'-0" high. Call for pricing on additional frame heights. * 14'-0", 16'-0", or 20'-0" high units available. * Two beam levels per unit. Call for pricing on additional beam levels. * Welded frames: 3" x 1-5/8" columns. * Capacity: 15,240 lbs per 48" of beam spacing * Beam Capacities   + 8'-0" : 4,521 lbs per pair   + 9'-0" : 3,232 lbs per pair   + 10'-0" : 3,054 lbs per pair * Units available with or without decking. Made in USA. *Lead time 2-3 days. FOB Chicago, IL 60639*. | | | | *Starter*  *Starter Kit*  *Add_on*  *Add-On Kit* | | | |
|  | STARTER UNIT INCLUDES  2 Frames, 4 Beams,  & 4 Wire Decks | | ADD-ON UNIT INCLUDES  1 Frame, 4 Beams,  & 4 Wire Decks | | | EXTRA SHELF INCLUDES  2 Beams,  & 2 Wire Decks | |
| **Upright**  **D x H** | **Product**  **No.** | **Wt. (lbs.)** | **Product**  **No.** | | **Wt. (lbs.)** | **Product**  **No.** | **Wt. (lbs.)** |
| **8’W UNITS WITH WIRE DECK (WT. CAP. 16,200 LBS.)\*** | | | | | | | |
| 36” x 96”  36” x 144” | POW401  POW403 | 262  304 | POW407  POW409 | | 217  238 | XS36096WD  XS36096WD | 86  86 |
| 42” x 96”  42” x 120”  42” x 144” | POW501  POW502  POW503 | 268  282  323 | POW507  POW508  POW509 | | 235  245  257 | XS42096WD  XS42096WD  XS42096WD | 94  94  94 |
| 48” x 96”  48” x 120”  48” x 144” | POW601  POW602  POW603 | 283  297  339 | POW607  POW608  POW609 | | 249  257  271 | XS48096WD  XS48096WD  XS48096WD | 100  100  100 |
| **9’W UNITS WITH WIRE DECK (WT. CAP. 16,200 LBS.)\*** | | | | | | | |
| 42” x 120”  42” x 144” | POW701  POW702 | 306  330 | POW705  POW706 | | 249  261 | XS42108WD  XS42108WD | 96  96 |
| 48” x 120”  48” x 144” | POW703  POW704 | 322  350 | POW707  POW708 | | 265  279 | XS48108WD  XS48108WD | 104  104 |
| **10’W UNITS WITH WIRE DECK (WT. CAP. 16,200 LBS.)\*** | | | | | | | |
| 42 x 120”  42 x 144” | HPOW801  HPOW802 | 346  370 | POW805  POW806 | | 289  301 | XS42120WD  XS42120WD | 116  116 |
| 48 x 120”  48 x 144” | HPOW803  HPOW804 | 358  386 | POW807  POW808 | | 301  315 | XS48120WD  XS48120WD | 122  122 |

*\*Capacity based on 48” beam spacing.*