|  |  |
| --- | --- |
| **Pallet Rack Storage System Kits*** One Starter Unit to begin each row. Add-On Units to extend or complete row.
* Unit Widths are 8'-0", 9'-0", and 10'-0".
* Unit Depths are 42" or 48". Call for pricing on 36".
* Uprights: 8'-0", 10'-0", or 12'-0" high. Call for pricing on additional frame heights.
* 14'-0", 16'-0", or 20'-0" high units available.
* Two beam levels per unit. Call for pricing on additional beam levels.
* Welded frames: 3" x 1-5/8" columns.
* Capacity: 15,240 lbs per 48" of beam spacing
* Beam Capacities
	+ 8'-0" : 4,521 lbs per pair
	+ 9'-0" : 3,232 lbs per pair
	+ 10'-0" : 3,054 lbs per pair
* Units available with or without decking. Made in USA. *Lead time 2-3 days. FOB Chicago, IL 60639*.
 | *Starter**Starter Kit**Add_on**Add-On Kit* |
|  | STARTER UNIT INCLUDES2 Frames, 4 Beams, & 4 Wire Decks | ADD-ON UNIT INCLUDES1 Frame, 4 Beams, & 4 Wire Decks | EXTRA SHELF INCLUDES2 Beams, & 2 Wire Decks |
| **Upright****D x H** | **Product****No.** | **Wt. (lbs.)** | **Product****No.** | **Wt. (lbs.)** | **Product****No.** | **Wt. (lbs.)** |
| **8’W UNITS WITH WIRE DECK (WT. CAP. 16,200 LBS.)\*** |
| 36” x 96”36” x 144”  | POW401POW403 | 262304 | POW407POW409 | 217238 | XS36096WDXS36096WD | 8686 |
| 42” x 96”42” x 120”42” x 144” | POW501POW502POW503 | 268282323 | POW507POW508POW509 | 235245257 | XS42096WDXS42096WDXS42096WD | 949494 |
| 48” x 96”48” x 120”48” x 144” | POW601POW602POW603 | 283297339 | POW607POW608POW609 | 249257271 | XS48096WDXS48096WDXS48096WD | 100100100 |
| **9’W UNITS WITH WIRE DECK (WT. CAP. 16,200 LBS.)\*** |
| 42” x 120”42” x 144” | POW701POW702 | 306330 | POW705POW706 | 249261 | XS42108WDXS42108WD | 9696 |
| 48” x 120”48” x 144” | POW703POW704 | 322350 | POW707POW708 | 265279 | XS48108WDXS48108WD | 104104 |
| **10’W UNITS WITH WIRE DECK (WT. CAP. 16,200 LBS.)\*** |
| 42 x 120”42 x 144” | HPOW801HPOW802 | 346370 | POW805POW806 | 289301 | XS42120WDXS42120WD | 116116 |
| 48 x 120”48 x 144” | HPOW803HPOW804 | 358386 | POW807POW808 | 301315 | XS48120WDXS48120WD | 122122 |

*\*Capacity based on 48” beam spacing.*