|  |
| --- |
| **Pallet Rack Wire Deck** |
|  |
|  | * **Step Channels fit in Step-down beams.**
* **Load capacities are based on evenly distributed loads.**

Step Channel Decks have (3) standard support channels that fit into the step-down ledges of the pallet rack beams. Call for pricing on flared channel wire deck. FOB Shipping Point. |
| **Product****No.** | **Length** | **Wt.****(lbs.)** | **Cap.\*\*****(lbs.)** |
| WD36463CWPI6 | 36 x 46” | 21 | 2,200 |
| WD42463CWPI6WD42523CWPI6WD42583CWPI6 | 42 x 46”42 x 52”42 x 58” | 242631 | 2,5002,5002,500 |
| WD48463CWPI6WD48523CWPI6WD48584CWPI6\* | 48 x 46”48 x 52”48 x 58” | 273336 | 2,5002,5002,500 |

\*48” x 58” wire decks have (4) channels to meet the 2,500 lbs. capacity.