|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Record Archive Shelving**  **• Convenient, economical bulk storage for record retention. • Units to 23' tall available with catwalks. Call for pricing. • 50% open wire decks available. • Assembles securely in minutes - no nuts or bolts needed.**  Rugged boltless construction provides for a cost efficient storage system. Rigid connections provide solid support for decking. 69" wide shelves with particle board will support 1,000 lbs. 42" wide shelves with particle board will support 600 lbs. based on UDL. Please call for weight capacities when using wire deck. Shelves adjust on 11⁄2" centers. Super strong posts are one piece construction. Available with solid particle board or 50% open wire decks. FOB Shipping Point. | | | | *RAS693007 With Wire Deck Option (boxes not included)* | | |
|  | | | | | *With Optional Shelf Decks* | |
|  |  | **FRAMEWORK ONLY** | | | **5/8” Particle Board**  *Add (Suffix PB)* | **Flat Wire Decks**  *Add (Suffix WD)* |
| **Size**  **W x D x H** | **No.**  **Levels** | **Product**  **No.** | **Weight**  **(lbs.)** | | **Weight**  **(lbs.)** | **Weight**  **(lbs.)** |
| 42” x 30” x 5’  69” x 30” x 5’ | 3  3 | RAS423005  RAS693005 | 41  63 | | 106  170 | 80  120 |
| 42” x 30” x 7’  69” x 30” x 7’ | 4  4 | RAS423007  RAS693007 | 61  92 | | 150  237 | 106  164 |
| 69” x 30” x 9’ | 5 | RAS693009 | 116 | | 297 | 205 |
| 69” x 30” x 11’\* | 6 | RAS6930011 | 148 | | 366 | 256 |

*\*Indicated Heavy Duty Angle Uprights Post. Note: 13’ and 15’ tall units are available. Please call for pricing.*

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Wide Span Bulk Racks **• Boltless bulk shelving is a low cost solution to your storage needs. • Assembles securely in minutes - no nut or bolts needed.**  Engineered for greater shelf loads, thanks to heavy gauge steel construction. Beams adjust on 11⁄2" centers. Wide shelves are rated at 550 lbs. for 4 ft. wide shelves, 600 lbs. for 6 ft. wide shelves per shelf level, evenly distributed. 8 ft. wide shelves are rated at 600 lbs. per shelf level, evenly distributed. One center support is included per pair of 72" and 96" wide beams. Capacities are based on use with particle board. Call for capacities using wire decking. Higher capacity beam styles, and taller units with additional storage levels are available -- call for details. Gray baked enamel finish. FOB Shipping Point. | | | *Basic 3 shelf unit – 7’ Tall (Framework, PB or Wire Decking)* | | | | | | |
|  | | | | | *With Optional Shelf Decks* | | | *Additional Shelves*  without Decking | |
|  |  | **FRAMEWORK ONLY** | | | | **5/8” Particle Board**  *Add (Suffix PB)* | **Flat Wire Decks**  *Add (Suffix WD)* |
| **Size**  **W x D x H** | **No.**  **Levels** | **Product**  **No.** | | **Weight**  **(lbs.)** | | **Weight**  **(lbs.)** | **Weight**  **(lbs.)** | **Product**  **No.** | **Weight**  **(lbs.)** |
| 48” x 24” x 7’  48” x 36” x 7’  48” x 48” x 7’ | 3  3  3 | A482407  A483607  A484807 | | 52  56  60 | | 112  147  181 | 84  101  119 | A4824SO  A4836S0  A4848SO | 11  12  14 |
| 72” x 24” x 7’  72” x 36” x 7’  72” x 48” x 7’ | 3  3  3 | A722407  A723607  A724807 | | 70  80  86 | | 161  216  268 | 118  170  203 | A7224SO  A7236SO  A7248SO | 17  20  24 |
| 96” x 24” x 7’  96” x 36” x 7’  96” x 48” x 7’ | 3  3  3 | A962407  A963607  A964807 | | 82  92  98 | | 203  273  341 | 146  206  245 | A9624SO  A9636SO  A9648SO | 21  24  26 |

*All 36” and 48” D wire decks are furnished with center support. 96” W unites are provided with two 48” W wire decks.*

**3 variations to choose from:**

* Units without decking (purchase decking locally)
* Units with particle board decking
* Units with 50% open wire decking (for fire codes)

**Boltless Storage Options**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| BEAM TYPES | | | | |
| **Space-Saving Shelving** | **Double Rivet Beams** | |
|  |  | |
| *Decking Available: Flat wire deck, particle board* | *Decking Available: Waterfall wire deck, particle board* | |
| DECKING TYPES | | | | |
|  | | |  | |
| **WIRE DECK**  Provides a durable open surface that allows for more air circulation and less dust accumulation. Waterfall style provided on double rivet beams. Flat style available for single rivet beams. | | | **PARTICLE BOARD**  An economical decking option that provides a durable, solid surface for medium to heavy duty storage applications. | |