|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Pallet Rack Wire Deck** | | | | |
|  | | | | |
|  | | * **Step Channels fit in Step-down beams.** * **Load capacities are based on evenly distributed loads.**   Step Channel Decks have (3) standard support channels that fit into the step-down ledges of the pallet rack beams. Call for pricing on flared channel wire deck. FOB Shipping Point. | | |
| **Product**  **No.** | **Length** | | **Wt.**  **(lbs.)** | **Cap.\*\***  **(lbs.)** |
| WD36463CWPI6 | 36 x 46” | | 21 | 2,200 |
| WD42463CWPI6  WD42523CWPI6  WD42583CWPI6 | 42 x 46”  42 x 52”  42 x 58” | | 24  26  31 | 2,500  2,500  2,500 |
| WD48463CWPI6  WD48523CWPI6  WD48584CWPI6\* | 48 x 46”  48 x 52”  48 x 58” | | 27  33  36 | 2,500  2,500  2,500 |

\*48” x 58” wire decks have (4) channels to meet the 2,500 lbs. capacity.